managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000000 00 00 00 00 00 0000 00 000000 00 00000000 b0 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		0

	converted data length field result: 
		0
got bad write pointer length!
	extracted write pointer from reply: 0x
vector::_M_range_check: __n (which is 3) >= this->size() (which is 0)