managing cmos1
in sync_send_buffer_commands_to_system()
got command for system. Sending...
00000000000000000000001a 06 67 01 7d 02 00000003 fe 0000 00 00000084 000004 ab 011085f0 02 
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000248 000004 63 
	requested remote write pointer
	got remote write pointer, reply length 20
received only 20 of data (26 requred):
	0x00 00 00 00 00 00 00 00 00 00 00 08 67 01 29 00 fe 00 00 22 
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
System does not contain requested buffer type: hk!
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 151
	type 			= hk
	payload.size() 		= 0
	system.name, .hex 	= cmos1, 14

in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000248 000004 78 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000000 00 00 00 00 00 0000 00 000000 00 00000000 b1 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		0

	converted data length field result: 
		0
got bad write pointer length!
	extracted write pointer from reply: 0x
vector::_M_range_check: __n (which is 3) >= this->size() (which is 0)
exiting
🦊:foxsi-4matter $ 
