managing cmos2
in sync_send_buffer_commands_to_system()
got command for system. Sending...
00000000000000000000001a 09 68 01 7d 02 00000003 fe 0000 00 00000020 000004 b1 011085f0 02 
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 
	requested remote write pointer
	got remote write pointer, reply length 20
received only 20 of data (26 requred):
	0x00 00 00 00 00 00 00 00 00 00 00 08 68 01 29 00 fe 00 00 9f 
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b714972a273a3648f658896898789b889799a7a8a2b8b1c8b6d8b1e8ccf8e0
stt:	0x0000
clk:	0x3355
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 190
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
	got remote write pointer, reply length 58
000000000000000000000011 68 01 09 00 fe 0000 00 000004 65 0010640262000000000000000000000011fe010d00fe0000000000040e004f8174 cb 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 10 64 02 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
expected 1825 bytes but received 0
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
creating DBE:
	last_packet_size:	796
	source_frame_size:	796
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()