managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000240 000004 85 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 


