managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 68 01 09 00 fe 0000 00 000004 65 0010aa00 38 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 10 aa 00 
	found cmos, swapped endianness
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 248
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cmos2, 15
	type 				= ql
	got pointer to pf: PacketFramer::
	frame_size 			= 492544
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 274
	packet_counter 			= 0
	system.name, system.hex 	= cmos2, 15
	type 				= ql
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
expected 1825 bytes but received 0
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b914972a263a344909588f68937890889799a0a8aeb8abc8acd8c2e8eff8e5
stt:	0x0000
clk:	0x9224
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 30
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
	got remote write pointer, reply length 1825
000000000000000000000715 68 01 09 00 fe 0000 00 000708 ae   5e 
	last header access: 24
	vector data length field result: 
		0
		0
		7
		8

	converted data length field result: 
		1800
got bad write pointer length!
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
creating DBE:
	last_packet_size:	796
	source_frame_size:	796
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000000 00 00 00 00 00 1c02 a0 005c02 a0 00000038 3b 
	last header access: 24
	vector data length field result: 
		0
		0
		92
		2

	converted data length field result: 
		23554
can't read past end of reply!
got bad write pointer length!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 02498264 1a 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x02 49 82 64 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
	got packet of size 1825 for frame with size 32400 and max size 32780. shrinking. 
	set frame packetizer frame
	packet framer frame.size(): 32780
	pushed ring buffer data to downlink buffer
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
	got remote write pointer, reply length 29
got malformed SpaceWire Ethernet header!
0xaa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa aa ef 
	last header access: 24
	vector data length field result: 
		0
		170
		170
		170

	converted data length field result: 
		11184810
can't read past end of reply!
got bad write pointer length!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for cdtede
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000248 000004 63 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0628824c 31 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x06 28 82 4c 
	found cmos, swapped endianness
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 297
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cmos1, 14
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 590848
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 329
	packet_counter 			= 0
	system.name, system.hex 	= cmos1, 14
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
expected 1825 bytes but received 0
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000248 000004 78 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 68 01 09 00 fe 0000 00 000004 65 00104004 d9 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 10 40 04 
	found cmos, swapped endianness
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 297
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cmos2, 15
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 590848
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 329
	packet_counter 			= 0
	system.name, system.hex 	= cmos2, 15
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
	got packet of size 1825 for frame with size 590400 and max size 590848. shrinking. 
	set frame packetizer frame
	packet framer frame.size(): 590848
	pushed ring buffer data to downlink buffer
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b614972a273a36490a588e688c7892889199b4a8bcb8a6c8c0d8abe8e2f8e4
stt:	0x0000
clk:	0x8243
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 296
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 005c82ac c5 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 5c 82 ac 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
	got packet of size 1825 for frame with size 32400 and max size 32780. shrinking. 
	set frame packetizer frame
	packet framer frame.size(): 32780
	pushed ring buffer data to downlink buffer
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
creating DBE:
	last_packet_size:	796
	source_frame_size:	796
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 02498264 1a 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x02 49 82 64 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte2, 10
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte2, 10
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0438824c 62 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x04 38 82 4c 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
	got packet of size 1825 for frame with size 32400 and max size 32780. shrinking. 
	set frame packetizer frame
	packet framer frame.size(): 32780
	pushed ring buffer data to downlink buffer
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0628824c 31 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x06 28 82 4c 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte4, 12
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte4, 12
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for cdtede
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000240 000004 85 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 68 01 09 00 fe 0000 00 000004 65 00101001 0e 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 10 10 01 
	found cmos, swapped endianness
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 248
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cmos2, 15
	type 				= ql
	got pointer to pf: PacketFramer::
	frame_size 			= 492544
	frame.size() 			= 484200
	frame_done 			= 0
	packets_per_frame 		= 274
	packet_counter 			= 269
	system.name, system.hex 	= cmos2, 15
	type 				= ql
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
	got packet of size 1825 for frame with size 491400 and max size 492544. shrinking. 
	set frame packetizer frame
	packet framer frame.size(): 492544
	pushed ring buffer data to downlink buffer
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b714972a263a3549155893688b7897889c999da8a1b8aec895d8a8e8f4f8e3
stt:	0x0000
clk:	0xd5aa
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 46
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 005c82ac c5 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 5c 82 ac 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
creating DBE:
	last_packet_size:	796
	source_frame_size:	796
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 02498264 1a 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x02 49 82 64 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte2, 10
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte2, 10
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0438824c 62 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x04 38 82 4c 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0628824c 31 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x06 28 82 4c 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte4, 12
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte4, 12
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for cdtede
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000248 000004 63 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000248 000004 78 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 68 01 09 00 fe 0000 00 000004 65 0010ac04 90 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 10 ac 04 
	found cmos, swapped endianness
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 297
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cmos2, 15
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 590848
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 329
	packet_counter 			= 0
	system.name, system.hex 	= cmos2, 15
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
		waiting to receive 1825 from system
	got packet of size 1825 for frame with size 590400 and max size 590848. shrinking. 
	set frame packetizer frame
	packet framer frame.size(): 590848
	pushed ring buffer data to downlink buffer
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b814952a263a3648fb588f689b789c88a3999ba8afb8b9c8b3d89ee8d8f8ef
stt:	0x0000
clk:	0x7ac8
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 238
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 005c82ac c5 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x00 5c 82 ac 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte1, 9
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
creating DBE:
	last_packet_size:	796
	source_frame_size:	796
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 02498264 1a 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x02 49 82 64 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte2, 10
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte2, 10
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0438824c 62 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x04 38 82 4c 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte3, 11
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
	got remote write pointer, reply length 29
000000000000000000000011 fe 01 0d 00 fe 0000 00 000004 0e 0628824c 31 
	last header access: 24
	vector data length field result: 
		0
		0
		0
		4

	converted data length field result: 
		4
	extracted write pointer from reply: 0x06 28 82 4c 
	got pointer to fp: FramePacketizer::
	header_size 			= 8
	frame.size() 			= 0
	max_packet_size 		= 2000
	packets_per_frame 		= 17
	packets_remaining_in_frame 	= 0
	system.name, system.hex 	= cdte4, 12
	type 				= pc
	got pointer to pf: PacketFramer::
	frame_size 			= 32780
	frame.size() 			= 0
	frame_done 			= 0
	packets_per_frame 		= 19
	packet_counter 			= 0
	system.name, system.hex 	= cdte4, 12
	type 				= pc
	static_strip_header_size 	= 24
	static_strip_footer_size 	= 1
	initial_strip_header_size 	= 0
	initial_strip_footer_size 	= 0
	subsequent_strip_header_size 	= 0
	subsequent_strip_footer_size 	= 0
write pointer has not advanced, skipping
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for cdtede
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000240 000004 85 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b714972a263a35491158a068937899889e99aaa89eb8acc89ad8b0e8d5f8df
stt:	0x0000
clk:	0x3cf1
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 244
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for cdtede
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000248 000004 63 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000248 000004 78 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b914962a263a34490b5888688f7899889d99b0a899b8a6c8bbd8b4e8d6f8df
stt:	0x0000
clk:	0xdba7
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 249
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for cdtede
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos1
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000240 000004 85 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000015 06 67 01 4d 02 00000003 fe 0000 00 00000100 000218 84 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing cmos2
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cmos2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000015 09 68 01 4d 02 00000003 fe 0000 00 00000240 000004 9e 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 44 ms
	waiting 356 ms
	waiting 44 ms
in sync_udp_receive_to_uplink_buffer()

managing housekeeping system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_command_to_system(), sending 0x01 f2 
in sync_send_command_to_system(), sending 0x02 f2 
in sync_send_command_to_system(), sending 0x04 20 
in sync_send_command_to_system(), sending 0x07 0b 
in sync_send_command_to_system(), sending 0x07 0f 
in sync_send_command_to_system(), sending 0x07 0e 
adc:	0x09b814972a273a354915589a68917887889799aea898b8b3c8a3d8a5e8def8de
stt:	0x0000
clk:	0x91c9
err:	0x0000
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
creating DBE:
	last_packet_size:	256
	source_frame_size:	256
	max_packet_size:	2000
	packets_per_frame:	1
in TransportLayerMachine::sync_udp_send_downlink_buffer()
in sync_send_command_to_system(), sending 0x01 f0 
in sync_send_command_to_system(), sending 0x02 f0 
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing timepix system
in sync_send_buffer_commands_to_system()
no commands in queue
	sending 0x8a
	sending 0x88
	sending 0x81
in sync_send_command_to_system(), sending 0x8a 
waiting for 1 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x88 
waiting for 27 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
in sync_send_command_to_system(), sending 0x81 
waiting for 4 B response
uart read timed out!
TransportLayerMachine::read() attempt 0 failed.
uart read timed out!
TransportLayerMachine::read() attempt 1 failed.
uart read timed out!
TransportLayerMachine::read() attempt 2 failed.
All TransportLayerMachine::read() attempts failed!
	sent all
	resized all
	resized all
creating DBE:
	last_packet_size:	0
	source_frame_size:	0
	max_packet_size:	2000
	packets_per_frame:	0
	buffered downlink
future exception in DownlinkBufferElement::set_this_packet_index for desired index 1. State: DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 0
	this_packet_index 	= 254
	type 			= tpx
	payload.size() 		= 0
	system.name, .hex 	= timepix, 13

	queued downlink
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	sent downlink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

system management fell through in Circle for uplink
	waiting 0 ms
	waiting 0 ms
	waiting 0 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte1 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte1
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0314 000004 8a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in sync_send_command_to_system(), sending 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 022b0000 00031c ab 
TransportLayerMachine::read() attempt 0 failed.
TransportLayerMachine::read() attempt 1 failed.
TransportLayerMachine::read() attempt 2 failed.
TransportLayerMachine::read() attempt 3 failed.
TransportLayerMachine::read() attempt 4 failed.
All TransportLayerMachine::read() attempts failed!
got wrong reply size!
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte2 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte2
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 041b0314 000004 7a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte3 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte3
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 060b0314 000004 2a 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()

managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
TransportLayerMachine::read_some() attempt 0 failed.
TransportLayerMachine::read_some() attempt 1 failed.
TransportLayerMachine::read_some() attempt 2 failed.
TransportLayerMachine::read_some() attempt 3 failed.
TransportLayerMachine::read_some() attempt 4 failed.
All TransportLayerMachine::read_some() attempts failed!
	got remote write pointer, reply length 0
received only 0 of data (26 requred):
	0x
in TransportLayerMachine::sync_udp_send_downlink_buffer()
	waiting 18 ms
	waiting 148 ms
	waiting 18 ms
in sync_udp_receive_to_uplink_buffer()
