^C
🦊:foxsi-4matter $ ./bin/formatter --verbose --config foxsi4-commands/systems.json 
log file: log/auto_2023-12-22_17:07:51.log
verbose printing on
running without UART interfaces.
reading file from foxsi4-commands/systems.json
finding systems...
adding new System:
	name:    gse
	id code: 0
	added an endpoint: (udp)192.168.1.118:9999
	no timing info provided for commanded system gse
adding new System:
	name:    downlink
	id code: 5
	added an endpoint: (tcp)224.1.1.0:8888
	no timing info provided for commanded system downlink
adding new System:
	name:    uplink
	id code: 6
	has uart!
adding new System:
	name:    formatter
	id code: 1
local endpoint: 192.168.1.8
	no timing info provided for commanded system formatter
adding new System:
	name:    housekeeping
	id code: 2
	added an endpoint: (tcp)192.168.1.16:7777
found item: intro
found item: pow
found item: rtd
adding new System:
	name:    power
	id code: 3
	no timing info provided for commanded system power
adding new System:
	name:    saas
	id code: 4
	no timing info provided for commanded system saas
adding new System:
	name:    cdtede
	id code: 8
	added an endpoint: (tcp)192.168.1.100:10030
adding new System:
	name:    cdte1
	id code: 9
	added an endpoint: (tcp)192.168.1.100:10030
found item: hk
found item: pc
adding new System:
	name:    cdte2
	id code: 10
	added an endpoint: (tcp)192.168.1.100:10030
found item: hk
found item: pc
adding new System:
	name:    cdte3
	id code: 11
	added an endpoint: (tcp)192.168.1.100:10030
found item: hk
found item: pc
adding new System:
	name:    cdte4
	id code: 12
	added an endpoint: (tcp)192.168.1.100:10030
found item: hk
found item: pc
adding new System:
	name:    timepix
	id code: 13
	has uart!
found item: tpx
adding new System:
	name:    cmos1
	id code: 14
	added an endpoint: (tcp)192.168.1.100:10030
found item: pc
found item: ql
adding new System:
	name:    cmos2
	id code: 15
	added an endpoint: (tcp)192.168.1.100:10030
found item: hk
found item: pc
found item: ql
adding new System:
	name:    broadcast
	id code: 254
	no timing info provided for commanded system broadcast
	adding commands for cmos1, 14...
	this Command was initialized as a read-command, but expects a zero-length reply
	added system commands to deck
	adding commands for timepix, 13...
	added system commands to deck
	adding commands for cdte4, 12...
	this Command was initialized as a read-command, but expects a zero-length reply
	added system commands to deck
	adding commands for cdte3, 11...
	this Command was initialized as a read-command, but expects a zero-length reply
	added system commands to deck
	adding commands for cdte2, 10...
	this Command was initialized as a read-command, but expects a zero-length reply
	added system commands to deck
	adding commands for cdte1, 9...
	this Command was initialized as a read-command, but expects a zero-length reply
	added system commands to deck
	adding commands for cdtede, 8...
	added system commands to deck
	adding commands for cmos2, 15...
	this Command was initialized as a read-command, but expects a zero-length reply
	added system commands to deck
	adding commands for housekeeping, 2...
	added system commands to deck
System does not contain requested buffer type: hk!
System does not contain requested buffer type: hk!
Timing for uplink: Timing::
	period 			= 1 ms
	command 		= 0 ms
	request 		= 0 ms
	reply 			= 1 ms
	idle 			= 0 ms
	retry_max_count 	= 1
	timeout 		= 10 ms
	intercommand_space 	= 3 ms

creating DBE:
	last_packet_size:	780
	source_frame_size:	32780
	max_packet_size:	2000
	packets_per_frame:	17
DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 17
	this_packet_index 	= 1
	type 			= pc
	payload.size() 		= 0
	system.name, .hex 	= cdte1, 9

set frame
DownlinkBufferElement::
	max_packet_size 	= 2000
	packets_per_frame 	= 17
	this_packet_index 	= 1
	type 			= pc
	payload.size() 		= 1992
	system.name, .hex 	= cdte1, 9

endpoints: 
uplink: 
uart: 
machine: 
trying to set ::reuse_address

