
managing cdte4 system
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_send_buffer_commands_to_system()
no commands in queue
in sync_remote_buffer_transaction() for cdte4
	can access ring buffer parameters
	write pointer width: 4
	sending read command: 000000000000000000000016 0102 fe 01 4d 02 00000103 fe 0000 00 07fb0314 000004 72 
	requested remote write pointer
	got remote write pointer, reply length 29
got malformed SpaceWire Ethernet header!
0x55 55 17 11 55 55 47 57 55 55 55 57 75 55 55 55 55 55 57 55 55 55 71 55 55 55 55 55 51 
	last header access: 24
	vector data length field result: 
		0
		85
		85
		113

	converted data length field result: 
		5592433
Segmentation fault
🦊:foxsi-4matter $ ./bin/formatter --verbose --config foxsi4-commands/systems.json 
